|  |
| --- |
|  |
| Two-Way with Single Clapper  **Function:** Used as an auxiliary inlet connection providing 500 GPM/1892 lpm minimum to supplement the fire protection water supply. Swing clapper provides unobstructed waterway. Exposed design is an economical method of satisfying fire dept inlet requirements.  **Regularly Furnished:** Cast brass two-way inlet body, swing clapper and pin lug swivel. Back or angle outlet as selected by model number. Lettering as selected. Size 4"/10.2cm X 2½" X 2½"/6.4cm X 6.4cm.  **Optional Finishes:**     **-B** Polished Brass     **-C** Rough Chrome Plated     **-D** Polished Chrome Plated  **Lettering Available:**              Auto Spkr or      Standpipe  **Specify:** Thread and lettering |
| <http://www.potterroemer.com/component/page,shop.product_details/flypage,shop.flypage/product_id,447/option,com_virtuemart/Itemid,4/> |