|  |
| --- |
|  |
| Two-Way with Single Clapper**Function:** Used as an auxiliary inlet connection providing 500 GPM/1892 lpm minimum to supplement the fire protection water supply. Swing clapper provides unobstructed waterway. Exposed design is an economical method of satisfying fire dept inlet requirements.**Regularly Furnished:** Cast brass two-way inlet body, swing clapper and pin lug swivel. Back or angle outlet as selected by model number. Lettering as selected. Size 4"/10.2cm X 2½" X 2½"/6.4cm X 6.4cm.**Optional Finishes:**    **-B** Polished Brass    **-C** Rough Chrome Plated    **-D** Polished Chrome Plated**Lettering Available:**             Auto Spkr or      Standpipe**Specify:** Thread and lettering |
| [http://www.potterroemer.com/component/page,shop.product\_details/flypage,shop.flypage/product\_id,447/option,com\_virtuemart/Itemid,4/](http://www.potterroemer.com/component/page%2Cshop.product_details/flypage%2Cshop.flypage/product_id%2C447/option%2Ccom_virtuemart/Itemid%2C4/) |